**DOVE REQUIREMENTS**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Order Information** | | | | | | |
| Project/Customer: |  | | | |  |
| Export Manager: |  | | | |  |
|  | | | | | | |
| **Luminaire Information** | | | | | | |
| Article: |  | | |  | | |
| Model number: |  | | |  | | |
| Quantity: |  | | |  | | |
| Luminous flux: |  | | | [lm] | | |
| Warranty: |  | | | [years] | | |
|  | | | | | | |
| **Screws** | | | | | | |
| Regular torx screws |  |  |  | |  | |
| Vandal proof screws |  |  |  | |  | |
| Screws must be colored |  |  |  | |  | |
|  |  |  |  | |  | |
| **End cap** | | | | | | |
| Both end caps mounted |  |  |  | |  | |
| One end cap mounted |  |  |  | |  | |
|  | | | | |  | |
| **Dimming** | | | | |  | |
| DALI |  |  |  | |  | |
| 1-10 V |  |  |  | |  | |
| Corridor function\* |  |  |  | |  | |
| \***Program needed** |  |  |  | |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Corridor Function parameters.** | | | | |
| Configuration type (choose one) | | | |  |
|  | | | |  |
|  | | | |  |
| Presence level: | | 100% |
| Absence level: | | 10% |
| Fade-in time: | | 00:00:00.000 |
| Fade-out time: | | 00:00:30.000 |
| Run-on time: | | 00:00:00 |
| Never off: | | YES |
|  | |  |
|  | | | | |
|  | | | | |
| Presence level | [1-100%] | |  |  |
| Absence level | [0-100%] | |  |  |
| Fade-in time | [0-9600s] | | **FIT** |  |
| Run-on time | [0-2550s] | | **ROT** |  |
| Fade-out time | [0-9600s] | | **FOT** |  |
| Switch-off delay | [0-2540s] | | **SOD** |  |
| *Never off* |  | |  | *If YES, then no SOD needed!* |

|  |
| --- |
| **Other Requirements** |
|  |