**LEAF SLIM REQUIREMENTS**

|  |
| --- |
| **Order Information** |
| Project/Customer: |  |  |
| Export Manager: |  |  |
|  |
| **Luminaire Information** |
| Article: |  |  |
| Model number: |  |  |
| Quantity: |  |  |
| Luminous flux: |  | [lm] |
| Warranty: |  | [years] |
|  |
| **Cables** |
| 2x1.5mm2 (x2.5m) open end |  |  |  |  |
| 5x1.5mm2 (x2.5m) open end |  |  |  |  |
| 2x1.5mm2 (x2.5m) with plug |  |  |  |  |
| 2x1.5mm2 (x2.5m) Wago Winsta (770-1172) 2-way plug |  |  |  |  |
| 5x1.5mm2 (x2.5m) Wago Winsta (770-1115) 5-way plug |  |  |  |  |
| 2x1.5mm2 (x2.5m) Ensto (NAC21S.W) 2-way plug |  |  |  |  |
| 5x1.5mm2 (x2.5m) Ensto (NAC51S.W) 5-way plug |  |  |  |  |
| Other |  |  |  |  |
|  |  |  |  |  |
| **Mounting** |
| Pre-mounted suspension details |  |  |  |  |
| Surface mount set |  |  |  |  |
| Other |  |  |  |  |
|  |  |  |  |  |

|  |
| --- |
| **Driver** |
|  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| **Loop through (Tridonic by default)** |
|  |
|  |  |  |
|  |  |  |
|  |  |  |
| **Dimming** |  |
| DALI |  |  |  |  |
| 1-10 V |  |  |  |  |
| Corridor function\* |  |  |  |  |
| \***Program needed** |  |  |  |  |

|  |
| --- |
| **Corridor Function parameters.** |
|  |  |
| Configuration type (choose one) |  |
|  |  |
|  |  |
| Presence level: | 100% |
| Absence level: | 10% |
| Fade-in time: | 00:00:00.000 |
| Fade-out time: | 00:00:30.000 |
| Run-on time: | 00:00:00 |
| Never off: | YES |
|  |  |
|  |
|  |
|  |  |  |  |
|  |  |  |  |
| Presence level  | [1-100%] |  |  |
| Absence level | [0-100%] |  |  |
| Fade-in time | [0-9600s] | **FIT** |  |
| Run-on time | [0-2550s] | **ROT** |  |
| Fade-out time | [0-9600s] | **FOT** |  |
| Switch-off delay | [0-2540s] | **SOD** |  |
| *Never off* |  |  | *If YES, then no SOD needed!* |

|  |
| --- |
| **Other Requirements**  |
|  |